Learning the Art of Electronics Labs - 4L.2 Emitter Follower Lab

# Test Circuit Description

*Art of Learning Electronics Labs (AoLEL) page 170 Figure 4L.3.*


### Circuit modifications

* The 1MΩ potentiometer was added between 33KΩ and VBase for dialing up Z source.  
  *Combined impedance to attenuate VE by 50% was measured to be 1.02 MΩ*
* Larger blocking capacitors 220µF were needed for 50 Hz. The 4.7µF specified were too small. *The 1KΩ load was filtered out @ 4.7µF having no effect on VE.*
* For R out F-Gen signal strength was too strong to meet the recommended 1 Volt p-p .

*1Vp-p and achieved with a voltage divider and using F-Gen’s -20dB Attenuation.*

* The clipping issue was resolved using the -15Vdc on the emitter’s load.  
  *All other ground points, including the scope probes connect to power supply common.*

|  |  |  |
| --- | --- | --- |
| Setting | Value | Comment |
| Frequency | 50 Hz |  |
| DC Offset | OFF |  |
| F-Gen | 1.92 Vp-p | 20 dB attenuation prior to voltage divider |



# Measurements

|  |  |  |  |
| --- | --- | --- | --- |
| Point | Condition | Vp-p | Amplitude |
| A | Baseline | 157 mV | 144 mV |
| V Base | Baseline | 160 mV | 136 mV |
| V Emitter | Baseline | 161 mV | 136 mV |
| *Input Resistance / Impedance Measurements* | | | |
| A | Zin Output 50% Attenuation | 158 mV | 144 mV |
| V Base | Zin Output 50% Attenuation | 80 mV | 50 mV |
| V Emitter | Zin Output 50% Attenuation | 74 mV | 49 mV |
| *Output Resistance / Impedance Measurements* | | | |
| A | Z out 1KΩ Load | 152 mV | 136 mV |
| V Base | Z out 1KΩ Load | 158 mV | 144 mV |

# Calculations & Assumptions

* ΔVin = ΔVout Voltage Gain of 1
* ΔI in << ΔI out Curren Gain much greater than 1
* Vin = Iin Rin (Ohms Law) and Rin = ΔVin / ΔI in
* Vout = I out Rout (Ohms Law) and Rout = ΔVout / ΔI out
* ß is not predictable. ß varies with Ic and temperature.
* ß ≈ 100 is the rule a thumb 2N3904 as safe *underestimation*.
* ΔVin = ΔVbase and ΔVout = ΔV Emitter.

#### Calculating Rin and Estimating ß by looking at Rin

* Compare amplitudes on both side of the R base (33 KΩ)  
  *The 1 MΩ potentiometer is dialed down to Zero.*
* *The 3.3KΩ REmitter is work around since the scope cannot measure current.*
* *Scope Measurements  
  144mV drop to 136mV is 5% loss. Keeping 95%.  
  Rin* = (95% / 5%) 33KΩ = 627 KΩ
* *Assuming ß = 100,* then Rin = ß Re  = 100 \* 3.3KΩ = 330 KΩ.  
  *in this case…*
* ß = 627 KΩ / 3.3 KΩ  
  ***ß = 190***

#### Calculating ß using the Hi Source Impedance measurement

* Compare amplitudes on both side of Rsource = 33KΩ + 1 MΩ
* Scope Measurements  
  144 mV drop to 50 mV is 65% loss, keeping only 35%  
  Rin = (35% / 65%) 1020 KΩ = 549 KΩ
* **ß = 166**

#### Calculating Rout

* Rout = R source/ß || R Emitter = Rin /ß || R Emitter
* ~~R~~~~out~~ ~~= (549KΩ/166) || 3.3KΩ = 1.65 KΩ~~
* ~~R~~~~out~~ ~~= (627KΩ/190) || 3.3KΩ = 1.65 KΩ~~
* **~~R~~~~out~~ ~~= 1.65 KΩ~~**
* Rout = (33KΩ/190) || 3.3KΩ = 165Ω
* Rout = (33KΩ/166) || 3.3KΩ = 187Ω
* **Rout = 165Ω to 187Ω**

#### 

# High Impedance Source Z Input (50% Attenuation on the Output V Emitter)

Graphical user interface

Description automatically generatedChart

Description automatically generated

## Measuring Output Impedance

#### Output Impedance Zout (Baseline)

#### Graphical user interface, application Description automatically generated

#### Output Impedance Zout (1KΩ load on V Emitter)

## A picture containing diagram Description automatically generated

## Workaround for Negative Side Clipping Vsource / Vinput

The negative side of the input signal is causing the Vbe to go negative and turn off the transistor.

Chart

Description automatically generated

Clipping stops when DC Offset shifts the entire signal above +0.62 Vdc.

A picture containing chart

Description automatically generated